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Warp knitted fabrics feature uniform stretch, balanced compressive strength, dimensional stability, and comfort. They are available in functional and sustainable forms, including single-layer, three-layer air/spacer structures, and composite materials.
[bookmark: heading_1]2. Material Composition
· Main fiber: Polyester (including recycled polyester/rePolyester), nylon (high-tensile)
· Recycled content available: 100% recycled polyester
· Monofilament connection for three-layer structures
[bookmark: heading_2]3. Structure & Style
· Three-layer air/spacer mesh (face and back connected by monofilament)
· Patterns: wavy, two-color seamless diamond, polka dot, single-sided diamond grid, quarter circle
· Types: high-density mesh, thin spacer mesh, stretch jersey, plain knit, heavy-duty mesh, gauze mesh
[bookmark: heading_3]4. Key Performance Properties
· Stretch: balanced equal stretch, double-sided stretch, elastic
· Comfort: breathable, lightweight, ultra-lightweight, soft and smooth
· Stability: good shape retention, high dimensional stability
· Durability: abrasion resistance, high tensile strength
· Functional treatments: water repellent, waterproof, moisture-wicking, mosquito repellent
· Composite: bondable with BIO rubber sponge
[bookmark: heading_4]5. Physical Specifications
· Thickness options: 1.0 mm, 3.0 mm
· Weight: 95 gsm (moisture-wicking single-sided plain knit)
[bookmark: heading_5]6. Typical Applications
· Active wear, sportswear
· Shoe materials
· Bags
· Home accessories
· Protective textiles
[bookmark: heading_6]7. Environmental Features
· Recycled polyester base fabrics
· Sustainable and eco-friendly production concept

